**3COM CORPORATION**

ETHERLINK II (3C503; ASSY.#7920)

|  |  |
| --- | --- |
| **NIC Type** | Ethernet |
| **Transfer Rate** | 10Mbps |
| **Data Bus** | 8-bit ISA |
| **Topology** | Star |
| **Wiring Type** | RG58A/U 50ohm coaxialAUI transceiver via DB-15 port |
| **Boot ROM** | Available |



|  |
| --- |
| **BOOT ROM ADDRESS** |
| **Address** | **JP7A** | **JP7B** | **JP7C** | **JP7D** | **JP7E** |
| » | Disabled | Closed | Open | Open | Open | Open |
|   | C8000h | Open | Closed | Open | Open | Open |
|   | CC000h | Open | Open | Closed | Open | Open |
|   | D8000h | Open | Open | Open | Closed | Open |
|   | DC000h | Open | Open | Open | Open | Closed |

|  |
| --- |
| **I/O BASE ADDRESS** |
| **Address** | **JP8A** | **JP8B** | **JP8C** | **JP8D** | **JP8E** | **JP8F** | **JP8G** | **JP8H** |
|   | 250h | Open | Open | Open | Open | Closed | Open | Open | Open |
|   | 280h | Open | Open | Open | Open | Open | Closed | Open | Open |
|   | 2A0h | Open | Open | Open | Open | Open | Open | Closed | Open |
|   | 2E0h | Open | Open | Open | Open | Open | Open | Open | Closed |
| » | 300h | Closed | Open | Open | Open | Open | Open | Open | Open |
|   | 310h | Open | Closed | Open | Open | Open | Open | Open | Open |
|   | 330h | Open | Open | Closed | Open | Open | Open | Open | Open |
|   | 350h | Open | Open | Open | Closed | Open | Open | Open | Open |

 **3Com Corporation**

 **EtherDisk Diskette for the EtherLink II Adapters**

 **System Resources**

 **Listed below are commonly used peripherals and their option settings. If any**

 **of these peripherals are installed in your computer, check which resources**

 **they are using and make sure that the software options on the EtherLink II**

 **adapters are not set to use the same resources. Other peripherals not**

 **mentioned in these lists could also cause conflicts.**

 **I/O Base Address Device**

 **---------------- ------**

 **200 Game I/O adapter**

 **270 LPT2: second parallel port**

 **2F0 COM2: second serial port**

 **320 Fixed disk adapter**

 **370 LPT1: primary parallel port**

 **380 Monochrome display adapter**

 **3C0 Enhanced graphics adapter**

 **3D0 Color graphics adapter**

 **Interrupt Level Device**

 **--------------- ------**

 **IRQ3 COM2**

 **IRQ4 COM1**

 **IRQ5 LPT2**

 **IRQ7 LPT1**

 **Memory Usage**

 **------------**

 **Address Device**

 **C0000-C3FFF EGA BIOS**

 **C0000-C8000 Normal VGA area**

 **C8000-CBFFF Hard disk adapter BIOS**

 **D0000-DFFFF EMS swap area (page frame)**

 **(%VER System Resources v3.4b)**